import time

time.sleep(0.1) # Wait for USB to become ready

print("Hello, Pi Pico!")

from machine import Pin

import utime

# Define the pin number to which the LED is connected

led\_pin = Pin(5, Pin.OUT)

# Blink the LED in a loop

while True:

led\_pin.toggle() # Toggle the LED state

utime.sleep(1) # Wait for 1 second

